ULTRASONIC WATER METER JOOBY JWM

Jooby Store Smart City Devices

Application

The ultrasonic water meter JOOBY JWM is designed for the accurate measurement of cold and hot water consumption in households, apartment buildings, commercial properties, and for the control of technological processes.

Part numbers

JWM2,5-110P-LRIR-T70

JWM4-130P-LRIR-T70

JWM6,3-150P-LRIR-T70

JWM2,5-110P-LRIR

JWM4-130P-LRIR

JWM6,3-150P-LRIR

Ordering specification

Example	Description
JWM2,5-110P-LRIR-Т70	Nominal flow rate Q3:2.5 – 2.5 m3/h;
2.5 – 2.5 m3/h;

4 – 4 m3/h; 6.3 – 6.3 m3/h. JWM2,5-110P-LRIR-Т70 Installation length: 110 – 110 mm; 130 – 130 mm; 150 – 150 mm. JWM2,5-110P-LRIR-Т70 Material of the hydraulic component: Р – Polymer; JWM2,5-110P-LRIR-Т70 Communication technology: LR – LoRaWAN®; IR – Infrared output pulse for the verification procedure. JWM2,5-110P-LRIR-Т70 Temperature class: T50, T70, T30/T70 – corresponding temperature class; without designation - T30.

Certificates and downloads

Certificate of conformity CE

Certificate of conformity UA

User Manual EN

User Manual UA

DataSheet EN

DataSheet DE

DataSheet UA