JOOBY AQUARIS RMS

Jooby Development Message documentation Message encoders/decoders Message encoders/decoders GUI (Demo) API for interacting with Jobby devices. Other documentation

JOOBY AQUARIS RMS 203 Radio module with sensor for Novator water meters. Installation. Activation

The red circle indicates the area where the magnet should be placed.

Determining the current state

Hold a magnet for 1 second

One short blink: the radio module is deactivated

Four short blinks: the radio module is activated

Activation / Deactivation

Bring and hold the magnet for 4-5 seconds

Remove the magnet immediately after a short blink

Wait for radio module response

Four short blinks: the radio module is activated, activation completed

One long and three short blinks: radio module is deactivated and it is necessary to activate it

Installation (Video)

Installation